You are here: CSP API Reference > 1 EXS & SwitchKit API Messages > Resource Modify 0x0125

Resource Modify 0x0125

SwitchKit Name

Resource Modify

Type

EXS and SwitchKit API message

Description

Resource Modify 0x0125

Use this message to change parameters for a processing resource in the CSP.

Sent by

Host application

Related API Message

Resource Create (0x0124)

Resource Delete (0x126)

Resource Connect (0x127)

SwitchKit Code

C Structure

typedef struct {

UBYTE AddrInfo[30];

UBYTE DataType;

UBYTE TLVCount;

UBYTE Data[221];

} XL_ResourceModify;

C Structure Response

typedef struct {

unsigned short Status;

UBYTE reserved6[13];

UBYTE AddrInfo[30];

UBYTE DataType;

UBYTE TLVCount;

UBYTE Data[219];

} XL_ResourceModify Ack;

C++ Class

class XLC_ResourceModify : public XLC_OutboundMessage {

public:

const UBYTE *getAddrInfo() const;

UBYTE *getAddrInfo();

void setAddrInfo(UBYTE *x);

XBYTE getConferenceID() const;

void setConferenceID(XBYTE x);

XBYTE getSpan() const ;

void setSpan(XBYTE x);

UBYTE getChannel() const ;

void setChannel(UBYTE x);

UBYTE getDataType() const;

void setDataType(UBYTE x);

UBYTE getTLVCount() const ;

void setTLVCount(UBYTE x) ;

UBYTE *getData() const ;

void setData(UBYTE *x) ;

};

C++ Class Response

class XLC_ResourceModifyAck : public

XLC_AcknowledgeMessage {

public:

unsigned short getStatus() const;

void setStatus(unsigned short x);

const UBYTE *getAddrInfo() const;

UBYTE *getAddrInfo();

void setAddrInfo(UBYTE *x);

XBYTE getConferenceID() const;

void setConferenceID(XBYTE x);

XBYTE getSpan() const ;

void setSpan(XBYTE x);

UBYTE getChannel() const ;

void setChannel(UBYTE x);

UBYTE getDataType() const;

void setDataType(UBYTE x);

UBYTE getTLVCount() const ;

void setTLVCount(UBYTE x) ;

const UBYTE *getData() const;

UBYTE *getData();

void setData(UBYTE *x);

};

EXS API Hex Format

MESSAGE (White) | RESPONSE (Gray)
Byte | Field Description | Byte | Field Description
0 | Frame (0xFE) | 0 | Frame (0xFE)
1, 2 | Length (0x00NN) | 1, 2 | Length (0x00NN)
3, 4 | Message Type (0x0125) | 3, 4 | Message Type (0x0125)
5 | Reserved (0x00) | 5 | Reserved (0x00)
6 | Sequence Number | 6 | Same Sequence Number
7 | Logical Node ID | 7 | Logical Node ID
8 : | AIB Address Method 0x00 - Individual AEs | 8, 9 | Status (MSB, LSB)
Number of AEs to follow | 10 : | AIB (same as message)
AEs 0x0D Channel 0x55 Conference ID 0x45 Child Conference ID | : | Data Type 0x00 TLVs
: | Data Type 0x00 TLVs | : | Number of TLVs to Follow
: | Number of TLVs to Follow | : | Mandatory Return TLVs 0x0602 Resource Type
: | TLVs | : | Checksum
| Mandatory TLVs 0x0602 Resource Type If the Resource Type is set to Send SMS (0x010A) or Receive SMS (0x010B): 0x0694 SMS Data Optional TLVs Optional TLVs if AIB is Conference and Resource Type is Conference or Child Conference: 0x0604 DTMF Clamping/Filtering Enable (Default is Disabled) 0x0607 Output Gain Control (Default is 0db) 0x0608 Noise Gating Enable (Default is disabled) 0x060A Echo Suppression Enable (Default is disabled) 0x060C Automatic Gain Control Enable (Default is disabled) Optional TLVs if AIB is Channel and Resource Type is Conference or Child Conference: 0x0604 DTMF Clamping/Filtering Enable 0x0607 Output Gain Control 0x0608 Noise Gating Enable 0x060A Echo Suppression Enable 0x060C Automatic Gain Control Enable 0x068B Input Gain Control Optional TLVs for Echo Cancel Parameters 0x0673 Echo Cancel Tap Length 0x0674 Echo Cancel NLP Type 0x0675 Echo Cancel ADAPT 0x0676 Echo Cancel Bypass 0x0677 Echo Cancel G.176 Modem Answer Detection 0x0678 Echo Cancel NLP Threshold 0x0679 Echo Cancel CNG Noise Threshold 0x067A Echo Cancel H Register Reset Optional TLV for Send SMS (0x010A) or Receive SMS (0x010B) 0x0695 FSK Modem Type
: | Checksum

A computer, attached to the Excel platform through an RS-232 or Ethernet link, from which you run the telecommunications application that controls the Excel platform.
A group of data bits in a specific format, with a flag at each end to indicate the beginning and the end of the frame.
See Address Information Block.
Most Significant Bit
Least Significant Bit
Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
Frequency Shift Keying