0x65 Global Object ID

The Object ID Address Element always comes after an Object Type and defines a specific instance of the Object Type. Each object has to give the range of valid IDs it can support.

Byte | AIB Field Description
--- | ---
0 | Address Element: 0x65
1 | Data Length: 0x02
2,3 | Data[0,1] Object ID Number

The information in an AIB that follows the header, down to the data field. An AIB can have one or more Address Elements. AEs correspond to Span, Channel, and SS7 Link.
See Address Information Block.