0x000E Terminating Span/Channel Offset

Used in:
0x1E Generic PPL ICB in Route Control message

Byte | Description
0, 1 | Tag 0x000E Terminating Span/Channel Offset
2, 3 | Length 0x0003
4 | Value[0] Offset

See Programmable Protocol Language.
See Information Control Block.
Range of channels provided by T1 or E1 transmission service. A physical span is a group of channels taking up a single physical wire. A logical span is a group of channels taking up less than a single logical wire, or carried over more than one physical wire.