0x000A Add Poll Interval

The poll interval, which is in 10 milliseconds, should be configured with values greater than 5. If configured with anything less than 5, the IP Signaling Series 3 card will automatically set the poll interval to 5.

Important! This poll is the IP Signaling Series 3 card to Matrix poll not the IP Signaling Series 3 card to Host poll.

Used in:
IP Signaling Series 3 Card Configure message (0x0100)
IP Signaling Series 3 Card Query message (0x0101)

Byte | Description
0, 1 | Tag 0x000A
2, 3 | Length 0x0004
4, 5 | Value[0-1] Number of Seconds Between Polls 0x00 - 0xFF In 10 millisecond units
6, 7 | Value[2-3] Number of Missed Polls Before Link is Declared Down 0x00 - 0xFF

Internet Protocol. Part of the TCP/IP family of protocols used to route messages and tracks the addresses of nodes.
A computer, attached to the Excel platform through an RS-232 or Ethernet link, from which you run the telecommunications application that controls the Excel platform.