0x0001 Add IP Signaling Series 3 Card

Used in:
Matrix Configure message (0x7D)
IP Signaling Series 3 Card Configure message (0x0100)

Byte | Description
0, 1 | Tag 0x0001
2, 3 | Length 0x0002
4 | Value[0] IP Signaling Series 3 Card ID, MSB 0x00
5 | Value[1] IP Signaling Series 3 Card ID, LSB 0x00-0x3F

Internet Protocol. Part of the TCP/IP family of protocols used to route messages and tracks the addresses of nodes.
Most Significant Bit
Least Significant Bit