You are here: CSP API Reference > 1 EXS & SwitchKit API Messages > Recorded Announcement File System Defragment 0x0103

Recorded Announcement File System Defragment 0x0103

SwitchKit Name

RecAnnFSDefrag

Type

EXS API and SwitchKit API message

Description

Recorded Announcement File System Defragment 0x0103

This message recovers unused memory in the file system used by the VRAS SIMM’s Flash memory on the DSP-ONE card. It is used after single Recorded Announcements (RANs) have been marked for deletion using the Recorded Announcement Single Delete (0x0117) message. The VRAS SIMM must first be taken out of service with the Service State Configure message. The host should wait for an Alarm message of "Recorded Announcement Defragment Complete" before bringing the VRAS SIMM in service. If defragmentation fails, the host receives an Alarm message of "Recorded Announcement File Defragmentation Failure" and the host should take action appropriate to the failure reason. The failure reason is in the Failure Code field of the Alarm message.

Sent by

Host

SwitchKit Code

C Structure

typedef struct {

UBYTE Slot;

UBYTE SIMM;

UBYTE reserved19[251];

} XL_RecAnnFSDefrag;

C Structure Response

typedef struct {

unsigned short Status;

UBYTE Data[251];

} XL_RecAnnFSDefragAck;

C++ Class

class XLC_RecAnnFSDefrag : public XLC_OutboundMessage {

public:

UBYTE getSlot() const;

void setSlot(UBYTE x);

UBYTE getSIMM() const;

void setSIMM(UBYTE x);

};

C++ Class Response

class XLC_RecAnnFSDefragAck : public XLC_AcknowledgeMessage {

public:

unsigned short getStatus() const;

void setStatus(unsigned short x);

const UBYTE *getData() const;

UBYTE *getData();

void setData(UBYTE *x);

};

EXS API Hex Format

MESSAGE (White) | RESPONSE (Gray)
Byte | Field Description | Byte | Field Description
0 | Frame (0xFE) | 0 | Frame (0xFE)
1, 2 | Length (0x000B) | 1, 2 | Length (0x0007)
3, 4 | Message Type (0x0103) | 3, 4 | Message Type (0x0103)
5 | Reserved (0x00) | 5 | Reserved (0x00)
6 | Sequence Number | 6 | Same Sequence Number
7 | Logical Node ID | 7 | Logical Node ID
: | AIB ( Address Method 0x00 - Individual AEs | 8, 9 | Status MSB, LSB 0x0B File System Conversion in Progress Trying to perform a VRAS function while the Flash memory on the VRAS SIMM is in the process of file system conversion. 0x0C Defragmentation in Progress Trying to perform a VRAS function while the Flash memory on the VRAS SIMM is defragmenting. 0x0E Invalid VRAS File System The Flash Memory File System does not support defragmentation.
Number of AEs | 10 | Checksum
AE 0x12 DSP SIMM
: | Checksum

Voice Recorded Announcement System
Quick depress and release of the phone plunger of a handset to signal the PBX or Centrex of instructions to follow (e.g., Call Transfer).
Digital Signal Processor
RAN. Recorded messages provided to callers for various reasons.
The condition of a component at a given instant. The current "context" of a PPL object, such as Idle, Seizing, Answered. In PPL files, a State is represented by a circle.
A computer, attached to the Excel platform through an RS-232 or Ethernet link, from which you run the telecommunications application that controls the Excel platform.
A group of data bits in a specific format, with a flag at each end to indicate the beginning and the end of the frame.
See Address Information Block.
Most Significant Bit
Least Significant Bit