0x01 Stage N Address Data

(Host-Supplied Digits)

Stage N Address Data ICBs use either host-supplied outpulsing or previously inpulsed digits. The format of the ICB depends on the type of digits you use.

The format of the Stage N Address Data ICB using host-supplied digits is as follows:

Used in:
Route Control message
Outseize Control message

ICB Type | 0x02 (Data)
ICB ID | 0x01
Data Length | Variable
Data[0] | Stage Number (1–4)
Data[1] | 0x01 (Host-Supplied Digits)
Data[2] | Outpulsing Signal Type 0x01 DTMF 0x02 MFR1 (host does not include KP or ST) 0x03 MFR2 0x04 MFR1 (host includes KP and any ST signal) 0x05 Dial Pulse
Data[3] | String Count (1 or 2)
Data[4] | String 1: BCD Digit Count
Data[5] | String 1: 1st BCD Digit Pair
: | :
: | String 1: Last BCD Digit Pair
: | String 2: BCD Digit Count
: | String 2: 1st BCD Digit Pair
: | :
: | String 2: Last BCD Digit Pair

A computer, attached to the Excel platform through an RS-232 or Ethernet link, from which you run the telecommunications application that controls the Excel platform.
See Information Control Block.
Outgoing call setup during real-time call processing on a specific channel.