0x027A SIP Registration Mode

Use this TLV to configure the CSP for different registration modes.

Used in:
VoIP Protocol Configure message
VoIP Protocol Query message

Byte | Description
0, 1 | Tag 0x027A
2, 3 | Length 0x0001
4 | Value[0] 0x00 Do not notify host (Default) All registrations are handled locally, without host intervention. 0x01 Notify host Registrations are stored locally, and the host is notified by a PPL Event Indication. The host has no control over the response generated. 0x02 Notify host and wait for response All registrations are added to the local database. The host is notified by a PPL Event Indication, and waits for a PPL Event Request before sending a response to the UA client. 0x03 Accept no registration

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
Voice over Internet Protocol. The delivery of voice information in digital form in discrete packets rather than in the traditional circuit-committed protocols of the public-switched telephone network (PSTN).
See Programmable Protocol Language.
A condition that, when met, drives a state machine from one state to another. A condition that drives a Component out of its current state by invoking an associated primitive.