0x36 MCC

The MCC Group and Channel components use the MCC address type. Currently, the MCC is always 0xFFFE.

Byte | AIB Field Description
--- | ---
2 | Address Element: 0x36
3 | Data Length: 0x02
4, 5 | Data[0, 1] Handle

See Address Information Block.
The information in an AIB that follows the header, down to the data field. An AIB can have one or more Address Elements. AEs correspond to Span, Channel, and SS7 Link.