0x05DD Server Address

Use this TLV to specify the name and location of the NFS server used for voice files. This TLV is used in the Generic Card Configure message and in the response to the Generic Card Query message.

Byte | Description
0, 1 | Tag 0x05DD Server Address
2, 3 | Length Variable
4, 5 | Value[0 ] Server ID (application-defined)
6-9 | Value[1 ] Primary IP Address (all zeros deletes the socket)
10, 11 | Value[2] Server Name Length
12-N | Value[3] Server Name
(2 bytes) | Value[4 ] Mount Name Length (max 32 bytes)
... | Value[5 ] Mount Name of Server

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
Internet Protocol. Part of the TCP/IP family of protocols used to route messages and tracks the addresses of nodes.