You are here: CSP API Reference > 1 EXS & SwitchKit API Messages > Local End Release Mode Configure 0x0021

Local End Release Mode Configure 0x0021

SwitchKit Name

LocalReleaseConfig

Type

EXS API and SwitchKit API message

Description

Local End Release Mode Configure 0x0021

This message sets a channel’s local end release mode, which determines whether a channel is released or parked when the other end of a connection releases.

Sent by

Host

SwitchKit Code

Configuration

LocalReleaseConfig (

Node = Integer,

Range = StartSpan : StartChannel - EndSpan : EndChannel,

ReleaseMode = Integer);

C Structure

typedef struct {

BaseFields Base;

unsigned short StartSpan;

UBYTE StartChannel;

unsigned short EndSpan;

UBYTE EndChannel;

UBYTE ReleaseMode;

} XL_LocalReleaseConfig;

C++ Class

class XLC_LocalReleaseConfig : public XLC_ChanRangeMessage {

public:

unsigned short getStartSpan() const;

void setStartSpan(unsigned short x);

UBYTE getStartChannel() const;

void setStartChannel(UBYTE x) ;

unsigned short getEndSpan() const;

void setEndSpan(unsigned short x);

UBYTE getEndChannel() const;

void setEndChannel(UBYTE x);

UBYTE getReleaseMode() const;

void setReleaseMode(UBYTE x);

};

EXS API Hex Format

MESSAGE (White) | RESPONSE (Gray)
Byte | Field Description | Byte | Field Description
0 | Frame (0xFE) | 0 | Frame (0xFE)
1, 2 | Length (0x00NN) | 1, 2 | Length (0x0007)
3, 4 | Message Type (0x0021) | 3, 4 | Message Type (0x0021)
5 | Reserved (0x00) | 5 | Reserved (0x00)
6 | Sequence Number | 6 | Same Sequence Number
7 | Logical Node ID | 7 | Logical Node ID
: | AIB Address Method 0x01 - Range of AEs | 8, 9 | Status (MSB, LSB)
10 | Checksum
Number of AEs to follow 0x02
AEs 0x0D Channel (Starting) 0x0D Channel (Ending)
: | Release Mode 0x01 Park Channel 0x02 Release Channel (Default) 0x03* Release Channel with Host Notify 0x04* Park Channel with Host Notify *These options work with T1 E&M Wink Start only. On Channels set with the Host Notify option, the Host receives the call processing event, Receive Idle. This option is valid for E&M trunk-type channels only.
: | Checksum

A computer, attached to the Excel platform through an RS-232 or Ethernet link, from which you run the telecommunications application that controls the Excel platform.
A group of data bits in a specific format, with a flag at each end to indicate the beginning and the end of the frame.
See Address Information Block.
Most Significant Bit
Least Significant Bit
Digital communications link - voice, data, and video at a 1.544 Mbps rate (24 64 Kbps channels)
Momentary interruption in a single frequency tone indicating the distant switch is ready to receive the digits just dialed.
In PPL, a condition that, when met, drives a state machine (PPL Component) from one state to another, by invoking an associated Primitive. In PPL files, an Event is marked by an arrow and text.