0x3D Ring Configuration Query

Use the Ring Configuration Query AIB to query ring configuration.

Important! If you attempt to query the ring configuration while another query is in progress, the Response Status will be 0x3F (Ring Configuration Query Already in Progress)

Byte | AIB Field Description
--- | ---
2 | Address Element: 0x3D
3 | Data Length: 0x01
4 | Data[0] Slot Number of EXNET® Card (Enter 0xFF to query all rings in the system)

See Address Information Block.
The information in an AIB that follows the header, down to the data field. An AIB can have one or more Address Elements. AEs correspond to Span, Channel, and SS7 Link.