You are here: PPL Developer’s Guide > 7 ISDN Atomic Functions > L3P BCC (0x0092) Atomic Functions

L3P BCC (0x0092) Atomic Functions

This section describes the atomic functions for the L3P BCC PPL component.

L3P BCC Atomic Functions

The following atomic functions are specific to the ISDN L3P BCC component.

AF Number | 51
Name | Send L3 ALLOCATION Request
Description | This function sends an Allocation Request to L3
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 52
Name | Send L3 ALLOCATION COMPLETE Request (AN only)
Description | This function sends an Allocation Complete Request to L3 (Allocation Confirm message specifying Allocation Complete)
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 53
Name | Send L3 ALLOCATION REJECT Request (AN only)
Description | This function sends an Allocation Reject Request to L3 (Allocation Confirm message specifying Allocation Reject)
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 54
Name | Send L3 DEALLOCATION Request
Description | This function sends a Deallocation Request message to L3
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 55
Name | Send L3 DEALLOCATION COMPLETE Request (AN only)
Description | This function sends a Deallocation Complete Request to L3 (Deallocation Confirm message specifying Deallocation Complete)
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 56
Name | Send L3 AUDIT Request (AN only)
Description | This function sends a AUDIT Request to L3
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 57
Name | Send Audit Complete to L3
Description | Sends Audit Complete message to Layer 3
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 58
Name | Test for User Port match in Audit Complete message
Description | Tests for User Port match in the Audit Complete message
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 59
Name | Send Clear Call Request to PSTN
Description | Sends a Clear Call Request to the PSTN
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 60
Name | Send PSTN Channel Request Ack
Description | This function sends a Channel Request Acknowledge message to PSTN
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 61
Name | Send PSTN Channel Request Reject
Description | This function sends a Channel Request Reject message to PSTN
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 62
Name | Send PSTN Channel Remove Ack
Description | This function sends a Channel Remove Acknowledge message to PSTN
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 63
Name | Send PSTN Channel Remove Reject
Description | This function sends a Channel Remove Reject message to PSTN
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 64
Name | Send PSTN Channel Indication Ack
Description | This function sends a Channel Indication Acknowledge message to PSTN
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 65
Name | Send Layer Manager Deferred Link Blocked Acknowledge
Description | Sends a Deferred Link Blocked Acknowledge to Layer Manager
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 66
Name | Send PSTN Channel Indication Reject
Description | This function sends a Channel Indication Reject message to the PSTN
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 68
Name | Send PSTN Channel Allocated Indication
Description | This function sends a Channel Allocated Indication message to PSTN
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 71
Name | Send PSTN Channel Allocation Reject
Description | Sends a Channel Allocation Reject to the PSTN
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 72
Name | Send PSTN a BCC Error Indication <Cause>
Description | Sends PSTN a BCC Error Indication
Arg1 | Cause: 1: Userport/Timeslot mismatch 2: Fault Message received from AN 3: Error Indication from Layer 3
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 75
Name | Send L4 Router Port Request
Description | This function sends a Port Request message to L4 Router
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 76
Name | Send L4 Router Reserve Port Request (AN only)
Description | This function sends a Reserve Port Request to L4 Router
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 77
Name | Check Status Indication for Reason
Description | Tests the Status Indication from L3 to determine if the reason specifies Audit Required
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 78
Name | Get BCC Reference Number
Description | Retrieves the BCC Reference Number
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 83
Name | Send PPL Event Indication with L4 Router reject status
Description | Tests the value of the reject status from L4 router and sends it to L5
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 84
Name | Send AN Fault Request to L3
Description | Sends a Fault Request to the peer entity; function is valid only on AN end
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 102
Name | Set the timeslot value from L4 incoming buffer
Description | This function sets the timeslot value equal to timeslot given in message from L4
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 104
Name | Set the timeslot value for this user port from V5.2 Timeslot/Userport table
Description | This function gets and sets the timeslot value from the user port ID by looking it up in the V5.2 Timeslots/Userport table
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 105
Name | Test the Error Code TLV in the message from PSTN
Description | This function tests the value of the Error Cause in the Error Code TLV in the incoming message from PSTN
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 106
Name | Test if we are LE
Description | Tests to determine if this V5 ID is LE or not
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | If LE: PPL Event INT Event 1 If AN: PPL Event INT Event 0

AF Number | 107
Name | Test if we are V5.2
Description | Tests to determine if this V5 ID is V5.2 or not
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | If LE: PPL Event INT Event 1 If AN: PPL Event INT Event 0

AF Number | 110
Name | Test the Response Status from L4RTR
Description | Tests the value of the Response Status TLV received from L4RTR
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | Success or Failure

AF Number | 111
Name | Test the More Response Status from L4RTR
Description | Tests the value of the More Response Status TLV received from L4RTR
Arg1 | <Not Used>
Arg2 | <Not Used>
Returns | Success or Failure

See Programmable Protocol Language.
See Integrated Services Digital Network.
See Atomic Function.
Protocol layer of the CSP.
The point in the Excel platform where a DS0 connects to a network. Also known as a "socket."
Public Switched Telephone Network
A condition that, when met, drives a state machine from one state to another. A condition that drives a Component out of its current state by invoking an associated primitive.
Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.