L3P PSTN Component PPL Timers (0x008B)

When specifying new timer values, remember that all PPL Timers are specified in 10 ms increments. For example, a PPL timer for 4 seconds is specified as 4000 (decimal, 400 x 10 ms = 4 seconds), which is the hexadecimal value of (0x190).

Timer ID | Description | Value (default)
--- | --- | ---
0x01 | Establish Acknowledge Wait (for first Establish only) | 2 seconds
0x02 | Establish Acknowledge Wait (for further Establish resends) | 5 seconds
0x03 | Disconnect Complete Wait | 2 seconds
0x04 | Status Wait | 2 seconds
0x05 | Signal or Protocol Parameter Received | 100 ms
0x06 | Signal Acknowledge Wait | 10 seconds
0x07 | Waiting for Disconnect Response | 4 seconds
0x08 | Waiting for Disconnect Request | 4 seconds
0x09 | Waiting for Datalink Connection Establish | 4 seconds

See Programmable Protocol Language.