0x067E Echo Cancel Comfort Noise Level

Use this TLV in the Resource Connect message to add comfort noise to RTP/ASR.

Byte | Description
0, 1 | Tag: 0x067E
2, 3 | Length: 0x0002
4, 5 | Value [0, 1] 0x0000 - 0x0059 Default - 0x0032 This value determines the initial level of the comfort noise. The higher this value is, the lower the added noise is. Dialogic does not recommend values 0x0000 - 0x001E.

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
Real-Time Transport Protocol. Supports transport of real-time data like interactive voice and video over packet-switched networks.