TCAP TUSI PPL Event Indications and Requests (ANSI)

Event ID | Event
--- | ---
0x04 | TC-UNI
0x05 | TC-U-ABORT
0x06 | TC-P-ABORT (Indication only)
0x07 | TC-QUERY-WITH-PERMISSION
0x08 | TC-QUERY-WITHOUT-PERMISSION
0x09 | TC-CONVERSATION-WITH-PERMISSION
0x0A | TC-CONVERSATION-WITHOUT-PERMISSION
0x0B | TC-RESPONSE
0x0C | TC-RESULT-L
0x0D | TC-RESULT-NL
0x0E | TC-U-ERROR
0x10 | TC-INVOKE-L
0x11 | TC-INVOKE-NL
0x12 | TC-U-REJECT
0x13 | TC-L-REJECT (Indication only)
0x1E | TCAP-RESTART
0x1F | TCAP MESSAGE NOT COMPLETE (Indication only)
0x18 | BAD REJECT RECEIVED FROM NETWORK
0x20 | TCAP DIALOG TIME OUT (Indication only)
0x21 | TCAP INITIATED ABORT (Indication only)
0x31 | TC-UNI-PRIMITIVE-SET
0x32 | TC-BEGIN-PRIMITIVE-SET
0x35 | TC-QUERY-WP-PRIMITIVE-SET
0x36 | TC-QUERY-WITHOUT PERMISSION PRIMITIVE SET
0x37 | TC-CONVERSATION WITH PERMISSION PRIMITIVE SET
0x38 | TC-CONVERSATION WITHOUT PERMISSION PRIMITIVE SET
0x39 | TC-RESPONSE PRIMITIVE SET

See Transaction Capability Application Part.