0x0C Socket Information

Used in:
0x00F1 IP Socket Query message

Byte | Description
0 | Tag 0x0C Socket Information
1 | Length 0x014
2 | Value[0] 0x00 Module (0xFF = Main Board)
3 | Value[1] Socket ID
4 | Value[2] Socket Status
5 | Value[3] Socket Client Flag 0x00 Server Side Socket 0x01 Client Side Socket
6-9 | Value[4-7] Local IP Address (4 bytes)
10, 11 | Value[8, 9] Local Port
12-15 | Value[10-13] Remote IP Address (4 bytes)
16, 17 | Value[14, 15] Remote Port
18-21 | Value[16-19] Socket User Name SASI Socket user is SASSI LHST Socket user is Local host communication module 0X00 00 00 00 Socket is not binded to any user

Internet Protocol. Part of the TCP/IP family of protocols used to route messages and tracks the addresses of nodes.
In SIP, an application program that sends SIP requests (See also Session Initiation Protocol). Clients may or may not interact directly with a person. Users agents and proxies contain clients (and servers).
Message delimiter (SS7 bit pattern - 01111110)
A 32-bit address, used in IP routing, which includes a Network address identifier assigned by a central authority and a Host ID (an end station identifier assigned by a LAN administrator).
The point in the Excel platform where a DS0 connects to a network. Also known as a "socket."