0xE001 Command

Used to supports M3UA functionality.

Used in:
NGA Configure message
NGA Service State Configure message

Byte | Description
0, 1 | Tag 0xE001
2, 3 | Length 0x0002
4, 5 | Value[0,1] 0x0000 - Add 0x0001 - Remove 0x0002 - Modify 0x0003 - Up 0x0004 - Down 0x0005 - In Service 0x0006 - Out of Service

The condition of a component at a given instant. The current "context" of a PPL object, such as Idle, Seizing, Answered. In PPL files, a State is represented by a circle.