BT IUP SPRC Configuration Bytes

Byte | Description | Value
0x28 | Number of samples in moving average | 100
0x29 | Instantaneous Onset Threshold for Incoming Calls. In units of 100ms | 1000 (10 ms)
0x2A | Moving Average Onset Threshold for Incoming Calls. In units of 100ms. | 500 (10 ms)
0x2B | Abatement Threshold for Incoming calls. In units of 100ms | 100 (10 ms)
0x2C | Number of samples to received before clearing Incoming congestion. | 10
0x2D | Instantaneous Onset Threshold for Outgoing Calls. In units of 100ms. | 1000 (10 ms)
0x2E | Moving Average Onset Threshold for Outgoing Calls. In units of 100ms. | 500 (10 ms)
0x2F | Abatement Threshold for Outgoing Calls. In units of 100ms. | 100 (10 ms)
0x30 | Number of samples to receive before clearing Outgoing congestion. | 10