You are here: CSP Developer’s Guide: Line Cards > 3 J1 Information > API Messages

API Messages

The following three API messages report ID numbers for the J-ONE cards:

• Card Population Query (0x07)

• Card Status Query (0x83)

• Card Status Report (0xA6)

The J-ONE and SJ1LC card ID numbers reported in the messages above are as follows:

• 0x0E: 4-span SJ1LC

• 0x1D: 8-span J-ONE card

• 0x1E: 16-span J-ONE card

• 0xDA: Standard J-ONE I/O card

• 0xDB: Redundant J-ONE I/O card

• 0xDC: Standby J-ONE I/O card