You are here: SwitchKit® Development Environment - TCAP Interface User’s Guide > 5 SwitchKit TCAP Abstraction Layer > sktal_recvTCAPComponent()

sktal_recvTCAPComponent()

Description

This method receives a TCAP component information from a SKTAL_EVENT.

Syntax

int sktal_recvTCAPComponent(int instanceId, SKTAL_EVENT *ev,

unsigned *dialogueId, SKTAL_CPT *cpt);

Input Parameters

Argument | Description
--- | ---
instanceID | Instance for given node/stack/SNN combination
ev | Event containing dialogue information

Input/Output Parameters

None

Output Parameters

Argument | Description
--- | ---
dialogueId | TCAP dialogue ID
cpt | Pointer to the structure containing component information

For definition see Appendix D, SKTAL_DLG and SKTAL_CPT Structure Definitions.

Return Value

SKTAL_SUCCESS: If method is successful.

SKTAL return code as defined in Appendix C, SKTAL Return Codes.

See Transaction Capability Application Part.