You are here: CSP Developer’s Guide: Internet Protocol > 3 IP Network Interface Series 2 Card > Fax Attributes

Fax Attributes

Overview

The IP Network Interface Series 2 card provides real-time fax relay, compliant with ITU T.38, over IP networks. This fax capability fully supports the ITU T.30 for Group 3 facsimile transmission protocol, with speeds of up to 14.4 Kbps. To remedy network packet loss and latency issues, the IP Network Interface Series 2 card employs fax spoofing techniques and packet redundancy schemes.

With the IP Network Interface Series 2 card, in the Fax Relay mode, faxes can be sent over IP using as much as 40 to 50 percent less bandwidth than the full 64 Kbps used on a traditional circuit-switched network.

The IP Network Interface Series 2 card also provides a Fax Bypass mode for real-time fax transmission using high-speed coders. If a matrix switchover occurs during fax transmission, the transmission fails.

Important! The IP Network Interface Series 2 card does not support the V.33 ITU Standard.

Configurable Fax Attributes

You can configure the following fax attributes.

Fax Type Enable

Fax Relay

The IP Network Interface Series 2 cards behavior depends upon how it is configured for detecting fax transmissions. When the host has configured a channel for Fax Relay modes and the IP Network Interface Series 2 card detects that a call is not a voice call, the codec switches from the Voice Coder mode to Answer Tone mode and then to Fax Relay mode. The packets are sent to the network as fax relay packets that comply with T.38. When the fax transmission ends, the channel reverts to Voice Coder mode.

Fax Bypass

When the host has configured a channel for bypass operation and a fax transmission is detected, the codec automatically switches from the current voice coder to the rate of the configured Coder Type. When the fax transmission ends, the channel reverts to Voice Coder mode.

Default: Disabled

TLV: 0x01C5 Fax Type Enable

0x00 Disable

0x01 Fax Relay

0x02 Fax Bypass

If the fax type is set to disabled, then the fax goes through as a voice call. Therefore, the fax transmission might not be successful depending on the codecs used.

Fax Bypass Coder Type

This attribute selects the codec to be used in a fax bypass scenario. Dialogic strongly advises selecting a data rate greater than 32 kbps.

Default: G.711 µLaw

TLV: 0x01C7 Fax Bypass Coder Type

Fax Payload Redundancy

Payload redundancy is a type of protection against network packet loss. By enabling redundancy, you can configure the CSP to send redundant packets to the network. For example, when you set the redundancy level to 2, the original payload is followed by two duplicate payload. Fax redundancy is supported in relay mode only.

Default: Disabled

TLV: 0x01D2 Fax Payload Redundancy

Source T.38 Port

This TLV is used to specify the local T.38 port number for fax relay. There is no default T.38 port value for this TLV. The host must select this port number as early as possible to ensure proper fax relay operation. If this port number is not specified in time, the fax relay fails. This TLV can be set during an active call.

Default: No default

TLV: 0x01E6 Source T.38 Port

Destination T.38 Port

This TLV is used to specify the remote T.38 port number for fax relay. There is no default T.38 port value for this TLV. The host must select this port number as early as possible to ensure proper fax relay operation. If this port number is not specified in time, the fax relay will fail. This TLV can be set during an active call.

Default: No default

TLV: 0x01E6 Destination T.38 Port

Internet Protocol. Part of the TCP/IP family of protocols used to route messages and tracks the addresses of nodes.
International Telecommunications Union (UN)
Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
The point in the Excel platform where a DS0 connects to a network. Also known as a "socket."