0x0618 Alarm Threshold Enabled Report

Use this TLV in the Generic Card Query message (0x0123).

Byte | Description
0, 1 | Tag: 0x0618 Alarm Threshold Enabled Report
2, 3 | Length: 0x0008
4 - 7 | Value[0-3]: A Bit Mask of Level 1 Alarms Enabled on this Card
8-11 | Value[4-7]: A Bit Mask of Level 2 Alarms Enabled on this Card

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.