0x0612 Connection Type

Use this TLV in the Connect with Data (0x0005) message to set up a one-way connection that is maintained during a matrix switchover. Do not use in the Connect (0x0000) message.

Use this TLV in the Resource Connect (0x0127) message to specify the connection type for a conferee.

Used in:
0x1E Generic PPL ICB in:
Connect with Data message
Resource Connect message

Byte | Description
0, 1 | Tag: 0x0612 Connection Type
2, 3 | Length: 0x0002
4, 5 | Value[0, 1]: Connection Type 0x0000 - 2-Way Connect (Default) 0x0001 - 1-Way Connect 0x0002 - 1-way Connect (Talk only)

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
See Programmable Protocol Language.
See Information Control Block.