You are here: CSP Hardware Product Descriptions > 3 Line Cards > Dialogic® E-ONE 75 Ohm I/O Card - EXSEIO1010/EXSEIO1010R

Dialogic® E-ONE 75 Ohm I/O Card - EXS-EIO-1010/EXS-EIO-1010R

Description

The Dialogic® E-ONE 75 Ohm I/O card connects the CSP to eight E1 lines and other telecommunications equipment.

Cable

Use only 75 Ohm impedance coaxial cable fitted with BNC connectors in compliance with ITU-T G.703.

Placement

The card resides in the rear card slots of a CSP 2090, CSP 2110 or CSP 2040 chassis.

Configuration Information

The part number, serial number, model number, and revision are located on the back of the board.

Specifications

The E-ONE 75 Ohm I/O card is designed to the following electrical, physical and environmental specifications.

Electrical | Specification
--- | ---
Supply Voltage, Vcc | 5.00V
Supply Current, Vcc @ 5.0V | 0.0A (typical)

Physical | Specification
--- | ---
Height | 318.5 mm (12.54 in.)
Depth | 105.2 mm (4.14 in)
Width | 19.7 mm (0.775 in.)

Environmental | Specification
--- | ---
Temperature - Storage | -40~C to 70~C (-40~F to 158~F)
Temperature - Operation | 0~C to 50~C (32~F to 122~F)
Temperature Shock - Storage | -40~C to 70~C to -40~C (-40~F to 158~F to -40~F) @ 5~C/min.
Temperature Shock - Operation | 0~C to 50~C (32~F to 122~F) @ 10~C/min.
Humidity - Operating | 5% to 85%
Altitude | Up to 4000 m (13,123 ft.)

Related Products

The products related to the E-ONE 75 Ohm I/O card are listed below.

Product | Model No. | RoHS Model No.
--- | --- | ---
E-ONE Card | EXS-E1C-1081 | EXS-E1C-1081R
E-ONE 75 Ohm Red I/O Card | EXS-EIO-1210 | EXS-EIO-1210R
E-ONE 75 Ohm Standby I/O Card | EXS-EIO-1310 | EXS-EIO-1310R

Front and Side Views

The front and side views show the span transmit/receive connectors.

A digital communications link - voice, data, and video at a 2.048 Mbps rate; 30B/2D or 31B/1D (ISDN); non-North American version of T1.
International Telecommunications Union (UN)
An I/O card that supports redundancy but has no external connections. A Standby I/O card sits behind whichever line card is originally designated as "standby." Compare to "Redundant I/O card" and "Standard I/O card."