0x01 Client Socket Register by IP

Used in:
IP Socket Configure message

Byte | Description
0 | Tag 0x01 Client Socket Register by IP
1 | Length 0x0E
2 | Value[0] 0x00 Module (0xFF = base board)
3 | Value[1] Socket ID
4-7 | Value[2-5] Local IP Address (4 bytes)
8, 9 | Value[6, 7] Local Port
10-13 | Value[8-11] Remote IP Address (4 bytes)
14, 15 | Value[12, 13] Remote Port

Internet Protocol. Part of the TCP/IP family of protocols used to route messages and tracks the addresses of nodes.
In SIP, an application program that sends SIP requests (See also Session Initiation Protocol). Clients may or may not interact directly with a person. Users agents and proxies contain clients (and servers).
A 32-bit address, used in IP routing, which includes a Network address identifier assigned by a central authority and a Host ID (an end station identifier assigned by a LAN administrator).
The point in the Excel platform where a DS0 connects to a network. Also known as a "socket."