You are here: CSP API Reference > 1 EXS & SwitchKit API Messages > Flash Timing Configure 0x0016

Flash Timing Configure 0x0016

SwitchKit Name

FlashTimingConfig

Type

EXS API and SwitchKit API message

Description

Flash Timing Configure 0x0016

Use this message to enable or disable flash detection and propagation on a channel or range of channels.

Sent by

Host

SwitchKit Code

Configuration

FlashTimingConfig (

Node = integer,

Range = StartSpan:StartChan - EndSpan:EndChan,

FlashMode = integer);

C Structure

typedef struct {

unsigned short StartSpan;

UBYTE StartChannel;

unsigned short EndSpan;

UBYTE EndChannel;

UBYTE FlashMode;

} XL_FlashTimingConfig;

C++ Class

class XLC_FlashTimingConfig : public XLC_ChanRangeMessage {

public:

unsigned short getStartSpan() const;

void setStartSpan(unsigned short x);

UBYTE getStartChannel() const;

void setStartChannel(UBYTE x);

unsigned short getEndSpan() const;

void setEndSpan(unsigned short x);

UBYTE getEndChannel() const;

void setEndChannel(UBYTE x);

UBYTE getFlashMode() const;

void setFlashMode(UBYTE x);

};

EXS API Hex Format

MESSAGE (White) | RESPONSE (Gray)
Byte | Field Description | Byte | Field Description
0 | Frame (0xFE) | 0 | Frame (0xFE)
1, 2 | Length (0x00NN) | 1, 2 | Length (0x0007)
3, 4 | Message Type (0x0016) | 3, 4 | Message Type (0x0016)
5 | Reserved (0x00) | 5 | Reserved (0x00)
6 | Sequence Number | 6 | Same Sequence Number
7 | Logical Node ID | 7 | Logical Node ID
: | AIB Address Method 0x01 Range of AEs | 8, 9 | Status (MSB, LSB)
10 | Checksum
Number of AEs to follow |  |
AEs 0x0D Channel (Starting) 0x0D Channel (Ending) |  |
: | Flash Mode 0x00 Flash Timing OFF 0x01 Flash Timing ON, propagate Flash to distant end 0x02 Flash Timing ON, send Call Processing Event message to the host. 0x03 Flash Timing ON, send Call Processing Event message to the host and propagate Flash to distant end.
: | Checksum

Quick depress and release of the phone plunger of a handset to signal the PBX or Centrex of instructions to follow (e.g., Call Transfer).
A computer, attached to the Excel platform through an RS-232 or Ethernet link, from which you run the telecommunications application that controls the Excel platform.
A group of data bits in a specific format, with a flag at each end to indicate the beginning and the end of the frame.
See Address Information Block.
Most Significant Bit
Least Significant Bit