0x0117 Alerting Propagation Mode

Use this TLV to indicate whether or not to suppress the automatic generation of the alerting signal by the CSP when the connected remote party sends out an alerting signal to the CSP. This TLV is for the SIP 180 message.

Used in:
0x1E Generic PPL ICB in:
PPL Event Request message
Connect with Data message

Byte | Description
0, 1 | Tag 0x0117
2, 3 | Length 0x0001
4 | Value[0] 1 Suppress alerting 2 Do not suppress alerting (default)

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
Session-Initiation Protocol. A signaling protocol used for establishing sessions in an IP network. A session could be a simple, two-way telephone call, or it could be a collaborative multi-media conference session.
See Programmable Protocol Language.
See Information Control Block.
A condition that, when met, drives a state machine from one state to another. A condition that drives a Component out of its current state by invoking an associated primitive.