You are here: CSP Hardware Product Descriptions > 7 Dialogic® CSP Expansion and Interconnect ONE I/O Card > Dialogic® CSP Expansion and Interconnect ONE I/O Card - EXS-XIO-1200/EXS-XIO-1200R

Dialogic® CSP Expansion and Interconnect ONE I/O Card - EXS-XIO-1200/EXS-XIO-1200R

Description

The EXNET-ONE I/O card controls node access to the EXNET® Ring and passes PCM data between nodes on the EXNET® Ring.

Placement

The card is installed into any CSP 2090, CSP 2110 or CSP 2040 I/O slot which does not have a corresponding line card. Install a Blockout Card in the corresponding slot in the front of the chassis. If any other card is installed in the front slot, the EXNET-ONE I/O card will not come in service and an alarm is sent to the host.

Configuration Information

The part number, serial number, model number, and revision are located on the back of the board.

Specifications

The EXNET-ONE I/O card is designed to the following electrical, physical and environmental specifications.

Electrical | Specification
--- | ---
Supply Voltage, Vcc | 5.00V
Supply Current, Vcc @ 5.0V | 4.41A (typical)

Physical | Specification
--- | ---
Height | 318.5 mm (12.54 in.)
Depth | 105.2 mm (4.14 in)
Width | 19.7 mm (0.775 in.)

Environmental | Specification
--- | ---
Temperature - Storage | -40~C to 70~C (-40~F to 158~F)
Temperature - Operation | 0~C to 50~C (32~F to 122~F)
Temperature Shock - Storage | -40~C to 70~C to -40~C (-40~F to 158~F to -40~F) @ 5~C/min.
Temperature Shock - Operation | 0~C to 50~C (32~F to 122~F) @ 10~C/min.
Humidity - Operating | 5% to 85%
Altitude | Up to 4000 m (13,123 ft.)

Related Products

The products related to the EXNET-ONE I/O card are listed below.

Product | Model No. | RoHS Model No.
--- | --- | ---
Debug Cable | Part # 64-0046-00 | Part # 164-0046-00

Front View

The front view shows the LEDs, push-button switches EXNET® fiber optic connectors, and Monitor port.

Controls and Indicators

The table below describes the LEDs and push button switches as shown in the front view of the EXNET-ONE I/O card.

LEDs | Color/Status | Description
--- | --- | ---
Det A | Red | Port A receiver does not detect signal
Green | Port A receiver detects signal, port is open
Green/Red | Port A receiver detects signal, port is looped back
Det B | Red | Port B receiver does not detect signal
Green | Port B receiver detects signal, port is open
Green/Red | Port B receiver detects signal, port is looped back
Stop | Red | EXNET-ONE I/O card has been aborted from the TDM bus.
Green | EXNET-ONE I/O card is running on the TDM bus.
Diag | Off | EXNET-ONE I/O card is idle
Green | Diagnostic has been completed successfully.
Red | Diagnostic has failed
Green/Red | Diagnostic is running
Push-button | Description
Abort | Stops card operation and takes the card off the bus.
Reset | Initiates a hardware reset of the card.

EXNET A and B Connectors

The table below indicates the fiber optic connector signals. Refer to the front view to locate these connectors.

Connector | Description
--- | ---
EXNET A |
RX | Receiver Connector (Input)
TX | Transmit Connector (Output)
EXNET B |
RX | Receiver Connector (Input)
TX | Transmit Connector (Output)

Monitor Port Pinouts

The table below indicates the pinouts of the Monitor port which is used for card test and debugging. Refer to the front view to locate this connector.

Pin | Description
--- | ---
1 | Receive
2 | Not Used
3 | Ground
4 | Transmit

Side View

The view shows the DIP switches and the jumpers.

DIP Switch S1

The table below describes DIP switch S1 settings. The shading (asterisk* for html documents) indicates factory-installed settings.

Position | Setting | Function
--- | --- | ---
1 | ON* | Disables Debug 1
OFF | Enables Debug 1
2 | ON* | Selects 9600 baud for monitor port
OFF | Selects 19200 baud for monitor port
3 | ON* | Disables Debug 2
OFF | Enables Debug 2
4 | ON* | Reserved for future use
OFF | Reserved for future use

DIP Switch S2

The table below describes DIP switch S2 settings. The shading (asterisk* for html documents) indicates factory-installed settings.

Position | Setting | Function
--- | --- | ---
1 | ON* | Reserved for future use
OFF | Reserved for future use
2 | ON | Reserved for future use
OFF* | API
3 | ON* | Reserved for future use
OFF | Reserved for future use
4 | ON* | Reserved for future use
OFF | Reserved for future use

Jumpers

The table below indicates the jumper settings.

Jumper | Setting | Description
--- | --- | ---
JP1 | Not Installed (default) | Factory use only
JP2 | Not Installed (default) | Factory use only
JP4 | Not Installed (default) | Factory use only
JP6 | Not Installed (default) | Factory use only

Excel's open architecture, proprietary, 1.3 Gbps fiber optic network using a packet-based protocol.
See Pulse Code Modulation.
The point in the Excel platform where a DS0 connects to a network. Also known as a "socket."
See Time Division Multiplexing.