You are here: SwitchKit® Development Environment Programmer’s Guide > 6 Handler Functions > sk_setTCAPHandler()

sk_setTCAPHandler()

Description

Use the sk_setTCAPHandler() function to organize the flow of TUSI and SUSI messages for your application. Once a stack and subsystem number have been assigned to an application, the sk_setTCAPHandler() function causes the specified handler function to be called whenever a CSP-initiated message arrives on a stack and subsystem number. This function does not affect the routing of any acknowledgment messages. This function is also available as skts_setTCAPHandler().

Syntax

int sk_setTCAPHandler(int aStackID, int anSSN, void *aTag, HandlerFunc* aHandlerFunc);

Threadsafe Syntax

int skts_setTCAPHandler(int aStackID, int anSSN, void *aTag, HandlerFunc* aHandlerFunc);

Parameters

The function parameters are shown in the table below.

Argument | Description
--- | ---
aStackID | Identifies Stack ID
anSSN | Identified Subsystem number
aTag | An application defined pointer which will be returned to the application when a handler is invoked.
aHandlerFunc | A pointer to a function that is designed to handle messages.

Return Values

Possible return values for this function:

OK | Always returns OK.