0x299A SIP Header Field Container

For SIP calls, this TLV contains the nested TLVs that in turn contain information regarding SIP Header Fields.

Used in:
0x0033 NPDI Universal ICB

This TLV uses the following nested TLVs:

• 0x299B SIP Header Field ID

• 0x299C SIP Header Field

Byte | Description
0, 1 | Tag 0x299A
2, 3 | Length Variable

Session-Initiation Protocol. A signaling protocol used for establishing sessions in an IP network. A session could be a simple, two-way telephone call, or it could be a collaborative multi-media conference session.
Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
Network Protocol Data Intelligence. Also called “Interworking,” it is a software product that operates within Excel’s Call Control (Layer 4) and Services (Layer 5) call processing layers. NPDI is meant to enhance Excel’s call processing product offering by allowing call processing layers (specifically Layers 4 and 5) to perform advanced analysis, generation, and conversion of Network Signaling (NS) Layer 3 information.
See Information Control Block.