0x066C Fax Processing Events Set Register

Used in: Generic Card Configure (0x0122) and Generic Card Query (0x0123) messages.

Byte | Description
0, 1 | Tag 0x066C Fax Processing Events Set Register
2, 3 | Length 0x0002
4, 5 | Value[0,1] Resgister Event Set (bitmask) (see details below) 0x0001 Phase A fax processing events 0x0002 Phase B fax processing events 0x0004 Phase C fax processing events 0x0008 Phase D fax processing events 0x0010 Phase E fax processing events 0x0020 Timer Events 0x0040 Data pump Events