0x31 SS7 Virtual CIC

Byte | AIB Field Description
--- | ---
2 | Address Element: 0x31
3 | Data Length: 0x07
4 | Data[0] Stack ID
5-8 | Data[1-4] DPC (4 Bytes)
9, 10 | Data[5, 6] CIC

See Address Information Block.
The information in an AIB that follows the header, down to the data field. An AIB can have one or more Address Elements. AEs correspond to Span, Channel, and SS7 Link.
Destination Point Code
See Circuit Identification Codes.