0x9043 Application Server Process

Used in:
NGA Configure message

Byte | Description
0, 1 | Tag 0x9043
2, 3 | Length Variable
4-n | Value[0,1] Primary IP Address
: | Value[2, 3] Secondary IP Address

Internet Protocol. Part of the TCP/IP family of protocols used to route messages and tracks the addresses of nodes.
A 32-bit address, used in IP routing, which includes a Network address identifier assigned by a central authority and a Host ID (an end station identifier assigned by a LAN administrator).