0x061C Server State

This TLV is included in the response of the Generic Card Query (0x0123) message in response to a DSP Series 2 General Card Configuration

Byte | Description
0, 1 | Tag: 0x061C - Server State
2, 3 | Length: 0x0003
4, 5 6 | Value[0]: Server ID (Application Defined) Value[1]: Server State 0x01 - Server is configured 0x02 - Server is connected 0x03 - Server is trying to connect 0x04 - Server is disconnected 0x05 - Server is disconnected urgent

.

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
Digital Signal Processor
The condition of a component at a given instant. The current "context" of a PPL object, such as Idle, Seizing, Answered. In PPL files, a State is represented by a circle.