MTP2 PPL Timers for other components (ITU)

PPL Component | Timer ID | Spec/Timer | Default Value (10 ms)
--- | --- | --- | ---
CC (0x0021) | 0x01 | Q-703/T5 | 10
IAC (0x0022) | 0x01 | Q-703/T2 | 1150
0x02 | Q-703/T3 | 150
0x03 | Q-703/T4N | 850
0x04 | Q-703/T4E | 60
LSC (0x0023) | 0x01 | Q-703/T1 | 4500

See Programmable Protocol Language.
Digital communications link - 44.378 Mbps rate
Digital communications link - voice, data, and video at a 1.544 Mbps rate (24 64 Kbps channels)