0x294F SIP Remote IP Port

This TLV reports the IP Port of the remote socket.

Used in:
0x0033 NPDI Universal ICB in:
Request for Service message

Byte | Description
0, 1 | Tag 0x294F
2, 3 | Length 0x0002
4-n | Value[0-n] MSB of the IP Port LSB of the IP Port

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
Internet Protocol. Part of the TCP/IP family of protocols used to route messages and tracks the addresses of nodes.
The point in the Excel platform where a DS0 connects to a network. Also known as a "socket."
Network Protocol Data Intelligence. Also called “Interworking,” it is a software product that operates within Excel’s Call Control (Layer 4) and Services (Layer 5) call processing layers. NPDI is meant to enhance Excel’s call processing product offering by allowing call processing layers (specifically Layers 4 and 5) to perform advanced analysis, generation, and conversion of Network Signaling (NS) Layer 3 information.
See Information Control Block.
Most Significant Bit
Least Significant Bit