0x01C2 Minimum Jitter Buffer Delay

The data in this TLV block are in millisecond units. The range of legitimate values is 0-150 milliseconds.

Used in:
0x1E and 0x001E Generic PPL ICBs in:
Resource Attribute Query message
Resource Attribute Configure message

Byte | Description
0, 1 | Tag 0x01C2 Minimum Jitter Buffer Delay
2, 3 | Length 0x0001
4 | Value[0] 0x00-0x96 ms ( 0x4B Default)

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
See Programmable Protocol Language.