0x04 Reset Indicator

At any time, the host can send a Reset Configuration message to the card to ensure that the IP address is assigned. The reset indicator value is returned in the Reset Indicator TLV. If the host sends a Reset or Engage TLV, an ACK is returned with all Indicator bits set to 0. If neither the Reset nor the Engage TLV is sent, the bit mask applies.

Used in:
IP Address Configure message

Byte | Description
0 | Tag 0x04 Reset Indicator
1 | Length 0x04
2 | Value[0] 0x00 Reset Indicator , MSB
3 | Value[1] Reset Indicator
4 | Value[2] Reset Indicator
5 | Value[3] Reset Indicator , LSB (0 = Disable, 1 = Enable) Bit 0: Main Board Bit 1: VoIP Module 1 Bit 2: VoIP Module 2 Bit 3: VoIP Module 3 Bit 4: VoIP Module 4 Bit 5: Reserved (0x00) Bit 6: Reserved (0x00) Bit 7: Reserved (0x00)

Internet Protocol. Part of the TCP/IP family of protocols used to route messages and tracks the addresses of nodes.
Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
Positive acknowledgment to a message
A 32-bit address, used in IP routing, which includes a Network address identifier assigned by a central authority and a Host ID (an end station identifier assigned by a LAN administrator).
Most Significant Bit
Least Significant Bit
Voice over Internet Protocol. The delivery of voice information in digital form in discrete packets rather than in the traditional circuit-committed protocols of the public-switched telephone network (PSTN).