0x0284 Resynchronize VoIP Media Parameter

Use this TLV to resynchronize VoIP media parameters (maintained locally by SIP and H.323 software) after the Resource Attribute Configure message is sent to the CSP to change the underlying VoIP media resource configuration.

Used in:
VoIP Protocol Configure message

Byte | Description
0, 1 | Tag 0x0284
2, 3 | Length 0x0001
4-7 | Value[0-3] 0 - No operation 1 - Resynchronize

0x0286 SIP Max Forwards

Used in:
VoIP Protocol Configure message
VoIP Protocol Query message

Byte | Description
0, 1 | Tag 0x0286
2, 3 | Length 0x0002
4,5 | Value[0] 0x00 - Disable 0x01 - Enable
: | Value[1] Variable (0x00-0xFF) Max-Forwards value

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
Voice over Internet Protocol. The delivery of voice information in digital form in discrete packets rather than in the traditional circuit-committed protocols of the public-switched telephone network (PSTN).
Session-Initiation Protocol. A signaling protocol used for establishing sessions in an IP network. A session could be a simple, two-way telephone call, or it could be a collaborative multi-media conference session.
ITU-T standard defines a set of call control, channel setup, and codec specifications for transmitting real-time voice and video over networks that do not offer guaranteed service or quality of service.