0x01E5 VoIP Resource Profile Assign

The Resource Profile Assign (0x01E5) TLV has been created to configure a module’s resource profile. Similar to changing the Gateway Mode, changing a VoIP module resource profile causes its TDM resources to change, causing the IP Network Interface Series 2 card to reset, so that new resources can be allocated.

Important! Changing the resource profile on any module causes the IP Network Interface Series 2 card host configuration to be reset.
You cannot mix VoIP resource profiles on the same
IP Network Interface Series 2 card or in the same chassis.

The Resource Profile Assign (0x01E5) TLV addresses the VoIP module by its module number. Since updating a VoIP module’s profile causes the IP Network Interface Series 2 card to reset, all of the modules can be reset in a single message.

The host has the flexibility to send one VoIP Resource Profile Assign TLV to assign the same resource profile to all modules or send multiple TLVs to individual modules. If any TLV is invalid, the message is negatively acknowledged (NACKED) and no action is taken.

Used in:
Resource Attribute Configure message

Byte | Description
0, 1 | Tag VoIP Resource Profile Assign (0x01E5)
2, 3 | Length 0x0003
4 | Value : Data [0] Module Number 0x00 Module 1 0x01 Module 2 0xFF All Populated VoIP Modules
5 | Value : Data [1] Profile Number 0x01 Profile 1 (IP Network Interface Series 2 - G.711 Only) 0x02 Profile 2 (IP Network Interface Series 2 - VDAC-ONE Compatibility.) 0x04 Profile 4 (IP Network Interface Series 3 - G.711 Only) 0x05 Profile 5 (IP Network Interface Series 3 - LBR+T.38)
6 | Value : Data [2] Force Flag 0x00 Update only if Spans have not been configured. 0xFF Update Unconditionally

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
A device that translates calls between an IP network and another network, typically the PSTN.
Voice over Internet Protocol. The delivery of voice information in digital form in discrete packets rather than in the traditional circuit-committed protocols of the public-switched telephone network (PSTN).
See Time Division Multiplexing.
Internet Protocol. Part of the TCP/IP family of protocols used to route messages and tracks the addresses of nodes.
Message delimiter (SS7 bit pattern - 01111110)