You are here: CSP API Reference > 3 Information Control Blocks > Data ICBs

Data ICBs

Hex | Data ICB Name | Used in These Messages
--- | --- | ---
0x01 | Stage N Address Data (Host-Supplied Digits) | Route Control, Outseize Control
0x02 | Stage N Address Data (Previously-Inpulsed Digits) | Route Control, Outseize Control
0x10 | ISDN Formatted IEs | Channel Release Request, Release Channel with Data, Request For Service With Data, Route Control, Outseize Control, PPL Event Indication, PPL Event Request
0x11 | ISDN Raw IEs | Channel Release Request, Release Channel with Data, Request For Service With Data, Route Control, Outseize Control, PPL Event Indication, PPL Event Request
0x12 | SS7 Parameters | Channel Release Request, Channel Released With Data, Connect With Data, Release Channel with Data, Route Control, Outseize Control, PPL Event Indication, PPL Event Request, Request For Service With Data
0x14 | PPL Argument 2 | PPL Event Request, PPL Event Indication
0x15 | DASS2/DPNSS Raw Data | Route Control, Outseize Control, Release Channel with Data, PPL Event Indication
0x16 | SS7 Protocol Violation | PPL Event Indication, PPL Event Request
0x17 | ISDN Formatted IEs with Event | Connect With Data
0x18 | ISDN Raw IEs with Event | Connect With Data
0x1A | Call Type | Outseize Control, Route Control
0x1C | SS7 TUP Formatted Fields | Route Control, Outseize Control, PPL Event Request, Release Channel with Data, Request For Service With Data, PPL Event Indication, Connect With Data
0x1E | Generic PPL ICB | PPL Event Indication, PPL Event Request, Route Control, Channel Release with Data
0x1F | SS7 Unformatted Raw Parameters | PPL Event Indication, Channel Release with Data, Release Channel with Data
0x20 | SS7 SCCP Parameters | PPL Event Indication, PPL Event Request
0x21 | SS7 TCAP Parameters | PPL Event Indication, PPL Event Request
0x22 | Raw SS7 Data Parameters |
0x23 | BT IUP Parameters | Channel Release with Data, Release Channel with Data, Request For Service With Data
0x24 | Product License | Product License Download
0x25 | ISDN Segmented | Outseize Control, Request For Service With Data, Release Channel with Data, Channel Release with Data, PPL Event Indication, PPL Event Request, Route Control
0x37 | Local CSP Matrix Series 3 Card Configuration Filename | TFTP Manage
0x38 | Local CSP Matrix Series 3 Card Server IP Address | TFTP Manage
0x39 | Adjacent CSP Matrix Series 3 Card Configuration Filename | TFTP Manage
0x3A | Adjacent CSP Matrix Series 3 Card Server IP Address | TFTP Manage
0x3B | Timestamp | TFTP Manage
0x3C | Save Options | TFTP Manage
0x3D | Load Version | TFTP Manage
0x3E | Load Filename | TFTP Manage
0x47 | Enable CSP-Initiated Messages | Multi-Host Configure
0x48 | Disable CSP-Initiated Messages | Multi-Host Configure
0x49 | Enable PPL Event Indication messages | Multi-Host Configure
0x4B | Deregister CSP-Initiated Messages | Multi-Host Configure
0x4C | Soft Register PPL Component IDs | Multi-Host Configure
0x50 | Hard Register All CSP Initiated Messages | Multi-Host Configure
0x51 | Soft Register All CSP Initiated Messages | Multi-Host Configure
0x52 | Deregister All CSP Initiated Messages | Multi-Host Configure
0x53 | Hard Register All PPL Component ID | Multi-Host Configure
0x54 | Soft Register All PPL Component IDs | Multi-Host Configure
0x55 | Deregister All PPL Component IDs | Multi-Host Configure
0x4A | Disable PPL Event Indication messages | Multi-Host Configure
0x5B | IP Signaling Series 3 Card ID | PPL Event Indication
0x5C | H.323 Hookflash Received (no data) | PPL Event Indication
0x5D | H.323 Signal Input Received | PPL Event Indication
0x5E | H.323 Signal Update Input Received | PPL Event Indication
0x5F | H.323 Alphanumeric Input Received | PPL Event Indication
0x62 | Remote Endpoints UII Capabilities | PPL Event Indication
0x65 | TCAP Primitive | PPL Event Indication, PPL Event Request
0x66 | SS7 Address Information | Request for Service with Data, Outseize Control
0xFF | PPL General Purpose Register Data | PPL Event Indication, PPL Event Request

In this section:

0x01 Stage N Address Data

0x02 Stage N Address Data

0x10 ISDN Formatted IEs

0x11 ISDN Raw IEs

0x12 SS7 Parameters

0x14 PPL Argument 2 Data

0x15 DASS2/DPNSS Raw Data

0x16 SS7 Protocol Violation Data

0x17 ISDN Formatted IEs With Event

0x18 ISDN Raw IEs with Event

0x1A Call Type

0x1C SS7 TUP Formatted Fields

0x1E Generic PPL

0x1F SS7 Unformatted Raw Parameters

0x20 SS7 SCCP Parameters

0x21 SS7 TCAP Parameters

0x22 Raw SS7 Data Parameters

0x23 BT IUP Parameters

0x24 Product License

0x25 ISDN Segmented Message

0x26 Channel Pad Value

0x37 Local CSP Matrix Series 3 Card Configuration Filename

0x38 Local Matrix Server IP Address

0x39 Adjacent CSP Matrix Series 3 Card Configuration Filename

0x3A Adjacent Matrix Server IP Address

0x3B Timestamp

0x3C Save Options

0x3D Load Version

0x3E Load Filename

0x47 Enable Switch-Initiated Messages

0x48 Disable Switch-Initiated Messages

0x49 Enable PPL Event Indication Messages

0x4A Disable PPL Event Indication Messages

0x4B Deregister Switch-Initiated Messages

0x4C Deregister PPL Components

0x50 Hard Register All Switch-Initiated Messages

0x51 Soft Register All Switch-Initiated Messages

0x52 Deregister All Switch-Initiated Messages

0x53 Hard Register All PPL Component IDs

0x54 Soft Register All PPL Component IDs

0x55 Deregister All PPL Component IDs

0x5B IP Signaling Series 3 Card ID

0x5D H.323 DTMF Signal Input Received

0x5E H.323 Signal Update Input Received

0x5F H.323 Alphanumeric Input Received

0x62 Remote Endpoints UII Capabilities

0x65 TCAP Primitive

0x66 SS7 Address Information

0xFF PPL General Purpose Register Data

See Information Control Block.
A computer, attached to the Excel platform through an RS-232 or Ethernet link, from which you run the telecommunications application that controls the Excel platform.
Outgoing call setup during real-time call processing on a specific channel.
See Integrated Services Digital Network.
RFS. A Status Message indicating that some entity is requesting service from the Excel platform.
See Programmable Protocol Language.
A condition that, when met, drives a state machine from one state to another. A condition that drives a Component out of its current state by invoking an associated primitive.
See Signaling System Number Seven.
Telephone User Part
See Transaction Capability Application Part.
Internet Protocol. Part of the TCP/IP family of protocols used to route messages and tracks the addresses of nodes.
A 32-bit address, used in IP routing, which includes a Network address identifier assigned by a central authority and a Host ID (an end station identifier assigned by a LAN administrator).
A programmable software component that uses PPL state machines that can be modified with the PPL Tool.
ITU-T standard defines a set of call control, channel setup, and codec specifications for transmitting real-time voice and video over networks that do not offer guaranteed service or quality of service.