0x01EE Invalid Packet Alarm Threshold

Indicates the alarming threshold for the number of invalid non-RFC 2833 packets received by the CSP. The CSP generates an alarm every time the number of invalid packets exceeds the threshold limit in a one-second period. The alarming is on a per RFC 2833 channel basis.

Used in:
VoIP Protocol Configure message
VoIP Protocol Query message

Byte | Description
0, 1 | Tag 0x01EE
2, 3 | Length 0x0002
4, 5 | Value[0,1] Number of invalid packets that justify alarm generation. 0x0000 - 0xFFFF 0x0032 is the default

Voice over Internet Protocol. The delivery of voice information in digital form in discrete packets rather than in the traditional circuit-committed protocols of the public-switched telephone network (PSTN).