L3 Global Call Reference Configuration Bytes

Byte | Description | Values
--- | --- | ---
0x01 | Channel ID encoding of extension bit | * 0x00 = Ext. bit set 0x01 = Ext. bit cleared
0x02 | N316: Number of RESTART attempts | 0x02
0x03 | Send FACILITY INDICATION to the host | * 0x00 = Disabled 0x01 = Enabled
0x04 | Send FACILITY ACK INDICATION to the host | * 0x00 = Disabled 0x01 = Enabled
0x05 | Send FACILITY REJECTED INDICATION to the host | * 0x00 = Disabled 0x01 = Enabled
0x06 | Send RESTART to the host | * 0x00 = Disabled 0x01 = Enabled
0x07 | Send RESTART ACK to the host | * 0x00 = Disabled 0x01 = Enabled
0x08 | Send STATUS to the host | * 0x00 = Disabled 0x01 = Enabled
0x09 | Send STATUS ENQUIRY to the host | * 0x00 = Disabled 0x01 = Enabled
0x0A | Send USER INFORMATION to the host | * 0x00 = Disabled 0x01 = Enabled
| * Default value |

Positive acknowledgment to a message