0x9051 Application Server State Query

Used in:
NGA Configure Query message
NGA State Notify message
NGA Service Query message

Byte | Description
0, 1 | Tag 0x9051
2, 3 | Length 0x0006
4 | Value[0] Application Service State 0x00 - Out of Service 0x01 - In Service
5, 6 | Value[1,2] Number of logical connections
7, 8 | Value[3,4 ] Logical Connection ID
9 | Value[5] Logical Connection State 0x00 - Out of Service 0x01 - In Service

The condition of a component at a given instant. The current "context" of a PPL object, such as Idle, Seizing, Answered. In PPL files, a State is represented by a circle.