0x0008 Criteria Type

Used in:
VoIP Protocol Configure message
VoIP Protocol Query message
0x1E and 0x001E Generic PPL ICBs in Route Control message

Byte | Description
0, 1 | Tag 0x0008 Criteria Type
2, 3 | Length 0x0002
4, 5 | Value[0, 1] 0x0000 Null 0x0001 - 0004 Address Digits 1, 2, 3, 4 0x0005 Time of day 0x0007 Incoming Channel 0x0010 Incoming Resource Group 0x001A Incoming Node 0x0065 Physical VoIP Channel 0x0071 Virtual VoIP Channel 0x03E9 - 03F8 User Defined 0x2710 - 0x4E20 Universal Protocol Data 0x2792 Source IP Address 0x27B4 IP Address Criteria 0x2A0E Media Connection Address

Voice over Internet Protocol. The delivery of voice information in digital form in discrete packets rather than in the traditional circuit-committed protocols of the public-switched telephone network (PSTN).
See Programmable Protocol Language.
Internet Protocol. Part of the TCP/IP family of protocols used to route messages and tracks the addresses of nodes.
A 32-bit address, used in IP routing, which includes a Network address identifier assigned by a central authority and a Host ID (an end station identifier assigned by a LAN administrator).