L3P SSUTR2 Configuration Bytes

Block 1

Byte | Description | Value
--- | --- | ---
0x01 | Host initiated OOS | 0=BLO/UBL (default) 1=RZC
0x02 | RAU reception processing options | 0=Auto reply w FIU (default) 1=PPL Event Indication RAU to Host (Host should send FIU)
0x03 | RFS Format | 0=SSUTR2 field format (default) 1=BCD encoded digits
0x04 | Send ACF PPL Event Indication to host | 0=Do not send (default) 1=Send event to host
0x05 | Send Answer PPL Event Indication to host | 0=Do not send (default) 1=Send event to host
0x06 | Congestion control check | 0=Congestion control disabled 1=Congestion control enabled (default)
0x07 | Specialized Circuit | 0=Mixed circuit (incoming/outgoing) (default) 1=Incoming calls only
0x0F | Field ID of called party address | 0x03
0x10 | Field ID of calling party address | 0x08
0x11 | Address indicator for calling line ID | 0
0x14 | No. of Fields in DEG | 1
0x15 | DEG message indicator field ID | 0x0D
0x16 | Field len | 0x01
0x17 | Field Data [0] | 0x01
0x1E | MIF No. of fields | 0x02
0x1F | Calling party category field ID | 0x01
0x20 | Field len | 0x01
0x21 | Field Data [0] | 0x0A
0x22 | MIF message indicator field ID | 0x02
0x23 | Field len | 0x02
0x24 | Field Data [0] | 0x00
0x25 | Field Data [1] | 0x00

Block 3

Byte | Description | Value
--- | --- | ---
0x01 | ACF No. of fields | 0x03
0x02 | ACF message indicator field ID | 0x0C
0x03 | Field len | 0x01
0x04 | Field Data [0] | 0x00
0x05 | ACF nature of access field ID | 0x18
0x06 | Field len | 0x01
0x07 | Field Data [0] | 0x01
0x08 | ACF circuit info field ID | 0x19
0x09 | Field len | 0x01
0x0A | Field Data [0] | 0x01

A computer, attached to the Excel platform through an RS-232 or Ethernet link, from which you run the telecommunications application that controls the Excel platform.
Out of Service
See Programmable Protocol Language.
See Request For Service.
A condition that, when met, drives a state machine from one state to another. A condition that drives a Component out of its current state by invoking an associated primitive.
In PPL, a condition that, when met, drives a state machine (PPL Component) from one state to another, by invoking an associated Primitive. In PPL files, an Event is marked by an arrow and text.