You are here: CSP Hardware Product Descriptions > 1 Chassis > Dialogic® Power Supply Card 60 Card - CSN-PSC-1000/CSN-PSC-1000R

Dialogic® Power Supply Card 60 Card - CSN-PSC-1000/CSN-PSC-1000R

Description

The Dialogic® Power Supply Card-60 (hereafter referred to as the PSC-60) supports the CSP 2040 chassis. A second PSC-60 card provides redundancy. During normal operation, the LED is ON. If the power module fails, the LED blinks.

This card converts the -48 V DC input power to +5 V DC using a power module. During normal operation, the power module LED is ON. If a module fails, the LED blinks. The switch enables or disables voltage conversion.

Placement

The card is installed into a dedicated Power slot on the front of the
CSP 2040 chassis.

Configuration Information

The part number, serial number, model number, and revision are located on the back of the board.

Specifications

The PSC-60 card is designed to the following electrical, physical and environmental specifications.

Electrical | Specification
--- | ---
Supply Voltage, Vcc | -48V
Supply Voltage, Vout | 5.00V
Supply Current, Vcc @ 5.0V | 60A (typical)

Physical | Specification
--- | ---
Height | 101.6 mm (4.0 in.)
Depth | 330.2 mm (13.0 in.)
Width | 28.6 mm (1.125 in.)

Environmental | Specification
--- | ---
Temperature - Storage | -40~C to 70~C (-40~F to 158~F)
Temperature - Operation | 0~C to 50~C (32~F to 122~F)
Temperature Shock - Storage | -40~C to 70~C to -40~C (-40~F to 158~F to -40~F) @ 5~C/min.
Temperature Shock - Operation | 0~C to 50~C (32~F to 122~F) @ 10~C/min.
Humidity - Operating | 5% to 85%
Altitude | Up to 4000 m (13,123 ft.)

Related Products

The products related to the PSC-60 card are listed below.

Product | Model No. | RoHS Model No.
--- | --- | ---
CSP 2040 Chassis | CSN-CHA-1112 | CSN-CHA-1112R

Front and Side Views

The front view shows the LEDs and switches used to generate, monitor and control +5 V DC for line card and I/O card use.

Controls and Indicators

The table below describes the LEDs and switches as shown in the front view of the PSC-60 card.

5V LED | Color/Status | Description
--- | --- | ---
| Green | Indicates normal operation of a power module
Blinking Green | Indicates a power module is out of tolerance or disabled
Off | Indicates a power module is turned off.
Switch | Description
ON | Enables conversion of -48 V DC to +5 V DC.
OFF | Disables conversion of -48 V DC to +5 V DC.

Important! In a redundant configuration the LEDs blinks when the associated power source (CB1 or CB2) or power switch on the card front panel is set to OFF.