0x061A AMD Parameters

Use this TLV in the Generic Card Configure message to set card-level parameters for Positive Voice Detection/Answering Machine Detection.

Byte | Description
0, 1 | Tag: 0x061A - AMD Parameters
2, 3 | Length: 0x0016
4, 5 | Value[0, 1]: Frequency Band 1 Minimum Detection Frequency (Hz) Min = 200 (0x00C8) Max = 3000 (0x0BB8) Default = 350 (0x015E) DISABLE = 0
6, 7 | Value[2, 3]: Frequency Band 1 Maximum Detection Frequency 1 (Hz) Min = 200 (0x00C8) Max = 3000 (0x0BB8) Default = 350 (0x015E) DISABLE = 0
8, 9 | Value[4, 5]: Frequency Band 2 Minimum Detection Frequency (Hz) Min = 200 (0x00C8) Max = 3000 (0x0BB8) Default = 750 (0x02EE) DISABLE = 0
10, 11 | Value[6, 7]: Frequency Band 2 Maximum Detection Frequency (Hz) Min = 200 (0x00C8) Max = 3000 (0x0BB8) Default = 1600 (0x0640) DISABLE = 0
12, 13 | Value[8, 9]: Frequency Band 3 Minimum Detection Frequency (Hz) Min = 200 (0x00C8) Max = 3000 (0x0BB8) Default = 1700 (0x06A4) DISABLE = 0
14, 15 | Value[10, 11]: Frequency Band 3 Maximum Detection Frequency (Hz) Min = 200 (0x00C8) Max = 3000 (0x0BB8) Default = 3000 (0x0BB8) DISABLE = 0
16, 17 | Value[12, 13]: Minimum Tone on time for declaration of tone present (10 ms) Min = 2 (0x0002) Max = 3000 (0x0BB8) Default = 15 (0x000F) DISABLE = 0
18, 19 | Value[14, 15]: Minimum Tone on time for declaration of tone not present (10 ms) Min = 2 (0x0002) Max = 3000 (0x0BB8) Default = 15 (0x000F) DISABLE = 0
20, 21 | Value[16, 17]: Minimum level of tone to declare present dBm Min = -54 (0xFFCA) Max = 3 (0x0003) Default = -20 (0xFFEC) DISABLE = 0l
22, 23 | Value[18, 19]: Minimum Voice on time for declaration of AMD_VOICE present (10 ms) Min = 2 (0x0002) Max = 3000 (0x0BB8) Default = 15 (0x000F) DISABLE = 0
24, 25 | Value[20, 21]: Minimum Voice off time for declaration of AMD_VOICE Not present (10 ms) Min = 2 (0x0002) Max = 3000 (0x0BB8) Default = 15 (0x000F) DISABLE = 0

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
Hertz