0x09CE Build Index Table

This TLV is used to activate configured GT entries. After the index table is built, all new added GT entries are in service and all deleted GT entries are out-of-service.

This TLV automatically activates the newly configured entries. After that, all GT entries that were pending to be added are brought into service. All GT entries that were pending to be deleted are brought out of service and internal entry space becomes available for subsequent configuration.

Used in:
SS7 SCCP TCAP Configure message

Byte | Description
0, 1 | Tag 0x09CE Build Index Table
2, 3 | Length 0x0001
4 | Value[0] 1 - Build Index All other values reserved for future use.

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
See Signaling System Number Seven.
See Transaction Capability Application Part.